Logo

Description automatically generated

Setup:

1. Ensure vehicle is turned off and parked safely
2. Fully open the hood and ensure it is secured
3. Locate the ECU in the firewall on the passenger’s side of the vehicle (See Green Arrow)



1. Disconnect all 3 of the ECU connectors. Be sure to release the locking tab (Green Arrow) before moving gray connector arm.

A picture containing indoor, several

Description automatically generated


1. Connect the ECU connector provided with the X4 to the ECU and to the SCT box
2. Connect the X4 to the SCT box using the OBDII cable
3. Connect the SCT box to the battery using the battery clamps provided

Tune Install:


1. Be sure to have the device setup using the steps above
2. On the X4 select Program Vehicle



1. Review and accept the Street Use Notice



1. If this is your first flash, select “Upload Stock”



1. Once started you will see “Saving Stock Data” run twice. This is normal.



1. Once you have uploaded stock select “Download Flash”



1. X4 will now program in the tune file. When complete reconnect the PCM.

Graphical user interface

Description automatically generatedText

Description automatically generated

Return to stock:

1. Be sure to have the device setup using the steps above
2. On the X4 select “Program Vehicle”



1. Review and accept the Street Use Notice


A picture containing text, electronics

Description automatically generated

1. Select “Return to Stock”



1. Confirm Return to Stock



1. X4 will now program in the stock file



1. When complete, reconnect PCM.

Text

Description automatically generated

LiveLink Gen-II

1. To use LiveLink with the 2021-2022 F150 please update to the current release version including any outstanding database updates.